Nama: Armando Budianto Djunaedi
Kelas: XII-TKJ 2
No. Absen: 6

Konfigurasi Hestia Control Panel

1. Setelah install debian 12 langkah selanjutnya login sebagai root dan ketik nano /etc/network/interfaces dan masukkan ip sesuai soal seperti berikut
80.80.80.xx
[image: ]
2. Kalau sudah restart jaringan dengan systemctl restart networking
3. lalu pergi ke menu edit > virtual network editor > vmnet8 lalu ganti subnet ip nya menjadi 80.80.80.0 habis itu apply dan oke
[image: ]
4. masuk ke nano /etc/resolv.conf tambahkan servername 8.8.8.8 dan servername 8.8.4.4, jika di resolv.conf sudah ada 8.8.8.8 dan 8.8.4.4 kita tidak usah tambahkan
5. kemudian masuk ke nano /etc/apt/sources.list dan tambahkan pagar pada kalimat di gambar bawah ini
[image: ]
6. lalu apt-get update dan tunggu sampai selesai
7. ketik nano /etc/ssh/sshd_login lau ganti hal hal berikut
#Port 22 🡪 Port 89
#PermitRootLogin prohibit-password 🡪 PermitRootLogin yes
8. habis itu systemctl restart sshd
9. masuk ke putty dengan port 89 hasil nya seperti berikut
[image: ] 
10.lalu kita install file hestia dengan perintah wget https://raw.githubusercontent.com/hestiacp/hestiacp/release/install/hst-install.sh
11.kalau kayak gini artinya sudah
[image: ]
12.lalu ketik perintah bash hst-install.sh lalu tunggu proses download sampai selesai
13.pilih y pada tampilan ini
[image: ]
14.masukkan email dan hostname yang valid pada bagian ini untuk hostname harus 3 oktaf seperti (hestia.mydomain.com),lalu enter dan tunggu
[image: ]
15.Lalu dibagian ini continue
[image: ]
16.lalu ketik perintah v-change-user-password admin ()
[image: ]


17.lalu login di web 80.80.80.19:8083
[image: ]
18.dan sudah berhasil masuk
[image: ]
19.Habis itu add 2 user baru yaitu pembeli 1 pembeli 2
[image: ]
20.lalu isi data yang dibutuhkan sperti name,contact,dan email
[image: ]
21.lalu save,dan begitupun yang user ke dua
22.habis itu pergi ke menu dns dan tambahkan dns 
[image: ]
23.yang ini pilih continue aja
[image: ]
24.isi domain nya dengan nama domain cp kita
[image: ]
25.lalu save



26.kembali ke menu user dan masuk ke pembeli 1
[image: ]
Pencet yang ini
[image: ]
27.Lalu tambahkan web domain
[image: ]
[image: ]
28.dns support dan mail support di centang
image19.png
Length: 223/ (2.3K) |text/plain]

saving to: ‘hst-install.sh’

hst-install.sh B )Y S ——

2024-09-19 22:59:55 (1.75 MB/s)

root@debian:~# |

‘hst-install.sh’ saved [4497/4497]
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Hestia Control Panel
1.8.12
www.hestiacp.com

Thank you for downloading Hestia Control Panel! In a few moments
we will begin installing the following components on your serve

- NGINX Web / Proxy Server

- Apache Web Server (as backend)

- PHP-FPM Application Server

- Bind DNS Server

- Exim Mail Server + SpamAssassin

- Dovecot POP3/IMAP Server

- MariaDB Database Server

- Vsftpd FTP Server

- Firewall (iptables) + Fail2Ban Access Monitor

Would you like to continue with the installation? [¥/N]: []
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Please enter admin email address: admin@example.com
Please enter FQDN hostname [debian]: hestia.example.com
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Made with love & pride by the open-source community around the world.
[ ! ] IMPORTANT: The system will now reboot to complete the installation process.
Press any key to continue[]
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Add DNS Zone

It s strongly advised to create a standard user account before adding a dns
domain to the server due to the increased privileges the admin account possesses
and potential security risks.

Add User Continue




image11.png
Add DNS Zone

hestia.example.com

IP Address

14.4.212172

Template BINDS
default

Advanced Options




image13.png
pembelil (pembeliT)

B embeliggmailcom

default 0 0.0mb/eo 0.0mb /oo




image12.png
-*)




image18.png
© Add Web Domain SORTBY: NAME 2 Applytoselected v = =

L Name IP Address Disk Bandwidth SsL Statistics




image10.png
Add Web Domain

Domain

IP Address

44212172

¥ DNS Support

¥ Mail Support




image2.png
# The primary netuork interface

auto ens33

iface ens33 inet static
address 80.80.80.19/24
gateuay 80.80.80.2




image4.png
B
& Virtual Network Editor X

Name  Type External Connection Host Connection  DHCP ‘Subnet Address

VMneto  Bridged  Auto-bridging - -
VMnet1  Host-only

Add Network... Remove Network | Rename Network...

VMnet Information
() Bridged (connect VMs directly to the external network)

Bridged to: Automatic Automatic Settings...

(© NAT (shared host's IP address with VMs) NAT Settings...

() Host-only (connect VMs internally in a private network)

{8 Connect a host virtual adapter to this network
Host virtual adapter name: VMware Network Adapter VMnets

(8 Use local DHCP service to distribute IP address to VMs. DHCP Settings...

Subnet P:[ 80 80 .80 . 0 | Subnet maskc 255.255.255. 0 |

Restore Defaults| | Import... Bxport, Ccancel Apply Help





image8.png
ebian GNU/Linux 12.7.9 _Bookworm_ - Official amdsd DVD Binary

with

irmuare

6240831-10:40]/ bookworm contrib main non

ree

irmuare




image3.png
EHCP Control panel 8§ (64) WhatsApp X >__(25) Payung Teduh - Untuk

2

PUTTY Security Alert

The hostkey is not cached for this server

80.80.80.19 (port 89)

Youhave no guarantee thatthe server is the computer you think itis.
The server's ssh-ed25519 key fingerprint s

ssh-ed25519 255 SHA256|EsBIOIFHDYoPSEVpcUTKzF Tz+Py TP5V1ef+sXIME

If you trustthis host press "Accept" o add the keyto PuTTY's cache and cary on connecting.

Ifyou wantto carry on connecting just once, without adding the key to the cache. press "Connect
Once"

Ifvou do nottrustthis host, press "Cancel" to abandon the connection

More info. Accept Connect Once





