KONFIGURASI FILE SERVER 
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1. Buatlah mesin dengan nama hostname nama kalian.
2. Download paket filenya:
[image: ]
3. Masuk kefile untuk mengubah sedikit konfigurasinya:
[image: ]
lalu keluar dengan ctrl+x.
4. Lalu restart dengan systemctl restart samba.
5. Lalu buat passwd user disambanya dengan:
[image: ]
6. Kalian bisa tes nya dengan buat mesin baru dengan desktop/gui, lalu bautlah satu jaringan dua mesin tersebut.
7. Pengetesannya dengan cara, pergi ketunar, lalu ketikan seperti ini:
[image: ]
Nanti akan dimintakan password dan user yang ingin kita gunakan. Dan selesai 
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root@debian:™# apt install samba
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comment = Home Directories

browseable = no

By default, the home directories are exported read-only. Change the

next parameter to 'no' if you want to be able to write to them.
read only = no

File creation mask is set to @796 for security reasons. If you want to
create files with group=rw permissions, set next parameter to 9775.
create mask = @709

Directory creation mask is set to 9709 for security reasons. If you want
create dirs. with group=rw permissions, set next parameter to @775.
directory mask = @700

By default, ““sserversusername shares can be connected to by anyone

with access to the samba serwver.

The following parameter makes sure that only ''username'' can connect
to Nhwserwverisusername

This might need tweaking when using external authentication schemes

to
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root@debian:™# smbpasswd -a user
New SMB password:

Retype new SMB password:
root@debian:™#
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